Arduino Reference - MouseIsPressed

Arduino

Reference Language | Libraries | Comparison | Changes

Mouse

## Mouse.isPressed()

#### Description

Checks the current status of all mouse buttons, and reports if any are pressed or not.

#### Syntax

Mouse.isPressed();
Mouse.isPressed(button);

#### Parameters

When there is no value passed, it checks the status of the left mouse button.

button: which mouse button to check - char

- MOUSE_LEFT (default)
- MOUSE_RIGHT
- MOUSE_MIDDLE

#### Returns

boolean : reports wether a button is pressed or not

#### Example

void setup(){
//The switch that will initiate the Mouse press
pinMode(2,INPUT);
//The switch that will terminate the Mouse press
pinMode(3,INPUT);
//Start serial communication with the computer
Serial1.begin(9600);
//initiate the Mouse library
Mouse.begin();
}
void loop(){
//a variable for checking the button's state
int mouseState=0;
//if the switch attached to pin 2 is closed, press and hold the right mouse button and save the state ina variable
if(digitalRead(2) == HIGH){
Mouse.press();
mouseState=Mouse.isPressed();
}
//if the switch attached to pin 3 is closed, release the right mouse button and save the state in a variable
if(digitalRead(3) == HIGH){
Mouse.release();
mouseState=Mouse.isPressed();
}
//print out the current mouse button state
Serial1.println(mouseState);
delay(10);
}
[Get Code]

#### See also

- Mouse.begin()
- Mouse.click()
- Mouse.end()
- Mouse.move()
- Mouse.press()
- Mouse.release()

Reference Home

Corrections, suggestions, and new documentation should be posted to the Forum.

The text of the Arduino reference is licensed under a Creative Commons Attribution-ShareAlike 3.0 License. Code samples in the reference are released into the public domain.

©Arduino | Edit Page | Page History | Printable View | All Recent Site Changes