Arduino Reference - KeyboardPress

Arduino

Reference Language | Libraries | Comparison | Changes

Keyboard

## Keyboard.press()

#### Description

When called, Keyboard.press() functions as if a key were pressed and held on your keyboard. Useful when using modifier keys. To end the key press, use Keyboard.release() or Keyboard.releaseAll().

It is necessary to call Keyboard.begin() before using press().

#### Syntax

Keyboard.press()

#### Parameters

char : the key to press

#### Returns

None

#### Example

// use this option for OSX:
char ctrlKey = KEY_LEFT_GUI;
// use this option for Windows and Linux:
// char ctrlKey = KEY_LEFT_CTRL;
void setup() {
// make pin 2 an input and turn on the
// pullup resistor so it goes high unless
// connected to ground:
pinMode(2, INPUT_PULLUP);
// initialize control over the keyboard:
Keyboard.begin();
}
void loop() {
while (digitalRead(2) == HIGH) {
// do nothing until pin 2 goes low
delay(500);
}
delay(1000);
// new document:
Keyboard.press(ctrlKey);
Keyboard.press('n');
delay(100);
Keyboard.releaseAll();
// wait for new window to open:
delay(1000);
}
[Get Code]

#### See Also

- Keyboard.begin()
- Keyboard.end()
- Keyboard.print()
- Keyboard.println()
- Keyboard.release()
- Keyboard.releaseAll()
- Keyboard.write()

Reference Home

Corrections, suggestions, and new documentation should be posted to the Forum.

The text of the Arduino reference is licensed under a Creative Commons Attribution-ShareAlike 3.0 License. Code samples in the reference are released into the public domain.

©Arduino | Edit Page | Page History | Printable View | All Recent Site Changes