Arduino Reference - Byte

Arduino

Reference Language | Libraries | Comparison | Changes

## byte

#### Description

A byte stores an 8-bit unsigned number, from 0 to 255.

#### Example

        byte b = B10010;  // "B" is the binary formatter (B10010 = 18 decimal)

#### See also

- word
- byte()
- Variable Declaration

Reference Home

Corrections, suggestions, and new documentation should be posted to the Forum.

The text of the Arduino reference is licensed under a Creative Commons Attribution-ShareAlike 3.0 License. Code samples in the reference are released into the public domain.

©Arduino | Edit Page | Page History | Printable View | All Recent Site Changes