/**
 * Copyright (c) 2009 Andrew Rapp. All rights reserved.
 *
 * This file is part of XBee-Arduino.
 *
 * XBee-Arduino is free software: you can redistribute it and/or modify
 * it under the terms of the GNU General Public License as published by
 * the Free Software Foundation, either version 3 of the License, or
 * (at your option) any later version.
 *
 * XBee-Arduino is distributed in the hope that it will be useful,
 * but WITHOUT ANY WARRANTY; without even the implied warranty of
 * MERCHANTABILITY or FITNESS FOR A PARTICULAR PURPOSE.  See the
 * GNU General Public License for more details.
 *
 * You should have received a copy of the GNU General Public License
 * along with XBee-Arduino.  If not, see <http://www.gnu.org/licenses/>.
 */
 
#include <XBee.h>

/*
This example is for Series 1 XBee
Sends a TX16 or TX64 request with the value of analogRead(pin5) and checks the status response for success
Note: In my testing it took about 15 seconds for the XBee to start reporting success, so I've added a startup delay
*/

XBee xbee = XBee();

unsigned long start = millis();

// allocate two bytes for to hold a 10-bit analog reading
uint8_t payload[] = { 0, 0 };

// with Series 1 you can use either 16-bit or 64-bit addressing

// 16-bit addressing: Enter address of remote XBee, typically the coordinator
Tx16Request tx = Tx16Request(0x1874, payload, sizeof(payload));

// 64-bit addressing: This is the SH + SL address of remote XBee
//XBeeAddress64 addr64 = XBeeAddress64(0x0013a200, 0x4008b490);
// unless you have MY on the receiving radio set to FFFF, this will be received as a RX16 packet
//Tx64Request tx = Tx64Request(addr64, payload, sizeof(payload));

TxStatusResponse txStatus = TxStatusResponse();

int pin5 = 0;

int statusLed = 11;
int errorLed = 12;

void flashLed(int pin, int times, int wait) {
    
    for (int i = 0; i < times; i++) {
      digitalWrite(pin, HIGH);
      delay(wait);
      digitalWrite(pin, LOW);
      
      if (i + 1 < times) {
        delay(wait);
      }
    }
}

void setup() {
  pinMode(statusLed, OUTPUT);
  pinMode(errorLed, OUTPUT);
  
  xbee.begin(9600);
}

void loop() {
   
   // start transmitting after a startup delay.  Note: this will rollover to 0 eventually so not best way to handle
    if (millis() - start > 15000) {
      // break down 10-bit reading into two bytes and place in payload
      pin5 = analogRead(5);
      payload[0] = pin5 >> 8 & 0xff;
      payload[1] = pin5 & 0xff;
      
      xbee.send(tx);

      // flash TX indicator
      flashLed(statusLed, 1, 100);
    }
  
    // after sending a tx request, we expect a status response
    // wait up to 5 seconds for the status response
    if (xbee.readPacket(5000)) {
        // got a response!

        // should be a znet tx status            	
    	if (xbee.getResponse().getApiId() == TX_STATUS_RESPONSE) {
    	   xbee.getResponse().getZBTxStatusResponse(txStatus);
    		
    	   // get the delivery status, the fifth byte
           if (txStatus.getStatus() == SUCCESS) {
            	// success.  time to celebrate
             	flashLed(statusLed, 5, 50);
           } else {
            	// the remote XBee did not receive our packet. is it powered on?
             	flashLed(errorLed, 3, 500);
           }
        }      
    } else {
      // local XBee did not provide a timely TX Status Response -- should not happen
      flashLed(errorLed, 2, 50);
    }
    
    delay(1000);
}
