Arduino Reference - LiquidCrystalPrint

Arduino

Reference Language | Libraries | Comparison | Changes

LiquidCrystal

## print()

#### Description

Prints text to the LCD.

#### Syntax

lcd.print(data)
lcd.print(data, BASE)

#### Parameters

lcd: a variable of type LiquidCrystal

data: the data to print (char, byte, int, long, or string)

BASE (optional): the base in which to print numbers: BIN for binary (base 2), DEC for decimal (base 10), OCT for octal (base 8), HEX for hexadecimal (base 16).

#### Returns

byte
print() will return the number of bytes written, though reading that number is optional

#### Example

#include <LiquidCrystal.h>
LiquidCrystal lcd(12, 11, 10, 5, 4, 3, 2);
void setup()
{
lcd.print("hello, world!");
}
void loop() {}
[Get Code]
Reference Home

Corrections, suggestions, and new documentation should be posted to the Forum.

The text of the Arduino reference is licensed under a Creative Commons Attribution-ShareAlike 3.0 License. Code samples in the reference are released into the public domain.

©Arduino | Edit Page | Page History | Printable View | All Recent Site Changes