Arduino Reference - KeyboardWrite

Arduino

Reference Language | Libraries | Comparison | Changes

Keyboard

## Keyboard.write()

#### Description

Sends a keystroke to a connected computer. If sending a numeric type, it sends it as an ASCII character (ex. Keyboard.write(97) will send 'a'). This is similar to pressing and releasing a key on your keyboard.

Only ASCII characters that are on the keyboard are supported. For example, ASCII 8 (backspace) would work, but ASCII 25 (Substitution) would not.

When sending capital letters, Keyboard.write() sends a shift command plus the desired character, just as if typing on a keyboard.

For a complete list of ASCII characters, see ASCIITable.com.

WARNING: When you use the Keyboard.write() command, the Arduino takes over your keyboard! Make sure you have control before you use the command. A pushbutton to toggle the keyboard control state is effective.

#### Syntax

Keyboard.write(character)

#### Parameters

character : a char or int to be sent to the computer. Can be sent in any notation that's acceptable for a char. For example, all of the below are acceptable and send the same value, 65 or ASCII A:

Keyboard.write(65); // sends ASCII value 65, or A
Keyboard.write('A'); // same thing as a quoted character
Keyboard.write(0x41); // same thing in hexadecimal
Keyboard.write(0b01000001); // same thing in binary (weird choice, but it works)
[Get Code]

#### Returns

int : number of bytes sent

#### Example

void setup() {
// make pin 2 an input and turn on the
// pullup resistor so it goes high unless
// connected to ground:
pinMode(2, INPUT_PULLUP);
Keyboard.begin();
}
void loop() {
//if the button is pressed
if(digitalRead(2)==LOW){
//Send an ASCII 'A',
Keyboard.write(65);
}
}
[Get Code]

#### See Also

- Keyboard.begin()
- Keyboard.end()
- Keyboard.press()
- Keyboard.print()
- Keyboard.println()
- Keyboard.release()
- Keyboard.releaseAll()
- ASCIITable tutorial

Reference Home

Corrections, suggestions, and new documentation should be posted to the Forum.

The text of the Arduino reference is licensed under a Creative Commons Attribution-ShareAlike 3.0 License. Code samples in the reference are released into the public domain.

©Arduino | Edit Page | Page History | Printable View | All Recent Site Changes